Data/hora: 03/06/2024 18:14:12

Biblioteca(s): | Epagri-Sede.
Tipo da produção científica: | Artigo em Anais de Congresso / Nota Técnica
Circulação/Nível: | -- - --
Data corrente: | 27/11/2012
Data da última atualização: | 27/11/2012
Autoria: | GARBOSSA, L. H. P.; VANZ, A.; SOUZA, R. V.; SOUZA, J. M.; RUPP, G. S.
Afiliação: | Epagri
Título: | Desenvolvimento de modelo de utilidade de marégrafo compacto de bóia e contrapeso com referência de nível.
Ano de publicação: | 2012
Fonte/Imprenta: | In: CONGRESSO BRASILEIRO DE OCEANOGRAFIA, 5., 2012, Rio de Janeiro. Anais... Rio de Janeiro: CBO, 2012.
Idioma: | Português
Conteúdo: | The implementation of the Florianopolis Bay hydrodynamics simulation demands water level time series. These dataset are obtained thru the use of two tide gauges. The tide gauges are located in the extreme North and South of Florianópolis Bay inlets. This paper presents the details about the installation and adaptations developed to settle the tide gauges in order to acquire good quality datasets. The equipment used to acquire the data is a mechanical pulley with a buoy and plummet device, connected to a data logger. The data logger is programmed to record the water level each fifteen minutes. In the South tide gauge a Radar equipment is also installed in order to compare the results. The R2 for the two tide gauges located at the same point in the South Bay is 0.995. The comparison of the results for the North and South tide gauges using R2 results in 0.888. The adaptations made to build the tide gauge resulted in a utility model that is capable of acquiring good quality data for hydrodynamic modeling.
Palavras-Chave: | Marégrafo; Modelo de utilidade; Nível do mar.
Categoria do assunto: | --
URL: | http://intranetdoc.epagri.sc.gov.br/producao_tecnico_cientifica/DOC_25901.pdf
Registro original: | Epagri-Sede (Epagri-Sede)
Exemplares: | Epagri-Sede - (91183-1) - UPC - PL - -- -  -  -  - DIS