Data/hora: 23/05/2024 11:00:33

Biblioteca(s): | Epagri-Sede.
Data corrente: | 01/03/2016
Data da última atualização: | 01/03/2016
Autoria: | SANTOS, A. H.
Título: | Experiment of Grain Drying.
Ano de publicação: | 1992
Fonte/Imprenta: | Tsukuba, Japão: Japan International Cooperation Agency, 1992.
Páginas: | 14 p.
Idioma: | Inglês
Conteúdo: | The following experiment was conducted in the attached farm of Tsukuba International Training Center and the objective was to compare three types of rice grain dryers.The three types of dryers were:flat bed dryer,circulating type dryer and solar grain dryer.The solar grain dryer was included in this experiment due to the good conditions available in Brazil to develop the same system.The result, in a rough analisys,was that the solar dryer is a more economic method than the others, because it absorbs the solar heat in a very efficient way. Despite the consumption of electricity,it is a very good and economic method to dry rice.In this experiment,there were some problems with very high temperature due to the very big area that was used to collect the solar heat. The temperature of the air in some points, reached to near 50ºC which caused some increase of light cracked grain.
Palavras-Chave: | circulating type dryer; flat bed dryer; rice; Solar grain dryer; vinyl house.
Categoria do assunto: | X Pesquisa, Tecnologia e Engenharia
URL: | http://intranetdoc.epagri.sc.gov.br/producao_tecnico_cientifica/DOC_36734.pdf
Registro original: | Epagri-Sede (Epagri-Sede)
Exemplares: | Epagri-Sede - (99972-1) - UPC - RT - DD -  -  -  - DIS